BAAA0013 - AIO Battery Firmware. (Load via USB next to DC Breaker)

Chipset v27 - HF21 actual Chipset update. Load via Uboot page, not the Device Manager page. Note DIP2/3 off for better stability during the load.

D619-A619 - Latest ARM/DSP for AIO1 via USB drive (DIP switch to 0000), or USB A-A cable method

GAAA0014 - Latest Gateway Update USB file with associated bconfig file

Test Pass Report

