AIO Inverter Manual Load Instructions
1. Get a blank USB Stick 8GB or less, formatted FAT32
2. Copy the 4 files provided, 1 x BCONFIG and 3 x .bin files. These are a set and must not be changed
3. Place the 4 files on the clean USB stick. Eject and remove from laptop
4. Fully power down the AIO2
5. Insert the USB into the top USB slot, marked AIO Upgrade
6. Power on the AIO. The USB will be scanned if present and files loaded to the flash memory
7. There will be a couple of reboots and the front panel LED will have numerous bouts of red/green flashing as each file is processed and loaded.
8. Final finished notification is a long continuous beep from the AIO. This is the cue to remove the stick. Upgrade is complete

AIO Dongle Manual Load instructions
1. Get a blank USB Stick 8GB or less, formatted FAT32
2. Copy the WirelessModule.bin file provided to the clean USB drive
3. Fully power down the AIO2
4. Insert the USB into the top USB slot, marked AIO Upgrade
5. Power on the AIO, which will also power on the dongle and load the update
6. Wait 5 mins. Then remove the stick.
7. Power cycle the AIO, to force the Dongle to reboot
8. Complete.

AIO2 Battery update
1. Get a blank USB Stick 8GB or less, formatted FAT32
2. Copy the 2 files provided, do not alter or rename them
3. place these 2 files on a clean USB stick
4. With the AIO powered up and battery on in normal operation
5. Insert the USB stick into the lower right slot, marked BCU Upgrade (Not the left LCD (Future Use))
6. you will hear 1 beep, to signal it can see the file
7. You will then hear the contactor open, and the battery FW will upgrade
8. On the 2nd beep, after approx. 1-2 mins. You may remove the USB
9. Upgrade complete. Battery will reboot itself and be back online in approx. 1-2 mins

GW Manual Update
1. Get a blank USB Stick 8GB or less, formatted FAT32
2. Copy the 2 files provided, do not alter or rename them
3. place these 2 files on a clean USB stick
4. With the GW powered down insert the USB stick in the upgrade slot. GW comms cable will need removal too
5. Power up the GW, from either mains, or the AIO via the comms cable
6. The GW will now update
7. When the GW has finished its update, remove the USB stick and power cycle the GW, to reboot the dongle from USB upgrade mode, to comms mode.

GW Dongle Manual Load instructions
1. Get a blank USB Stick 8GB or less, formatted FAT32
2. Copy the WirelessModule.bin file provided to the clean USB drive
3. Fully power down the GW
4. Insert the USB into the USB upgrade slot
5. Power on the GW, from any source
6. Wait 5 mins. Then remove the stick.
7. Power cycle the GW, to force the Dongle to reboot
8. Complete.